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1)
Identification of the substance/preparation and the company:


Product Information:


Trade Name:
Hungarian Paraffin Wax Slab & Pellets


52/54


CAS No: 64742-43-4      EINECS No: 265-145-6


Supplier:
Meade-King, Robinson & Co. Ltd


2nd Floor, Tower Building 


22, Water Street, LIVERPOOL, L3 1BL



Tel: 0151 236 3191   Fax: 0151 236 4431

​​​​​​​​______________________________________________________________________________________________________
2)
Hazard Identification:

This product is not classified as hazardous.

Physicochemical hazards: Clothes or paper contaminated with wax constitute a fire hazard.  Spilled wax can make floors 


slippery.


Health hazards: Hot wax may cause burns.  Avoid repeated and prolonged contact.  Inhalation of hot wax vapours may irritate the upper respiratory tract and cause coughing.


Environmental hazards: Prevent hot wax from entering drain systems as it can cause blockages after cooling.

______________________________________________________________________________________________________
3)
Composition/information on ingredients:

Chemical Characterisation:


Paraffin Wax -
solid saturated hydrocarbons Cn  H2n  + 2 where C= 20 – 50



Synonym -  petroleum wax 

______________________________________________________________________________________________________


4)
First Aid measures:


Immediate measures:
solid
none



liquid
same action as in case of burn



Eye contact
liquid
flush eyes with cold water.  Seek medical  




attention


Skin contact
liquid
immerse the area in water to assist cooling.




Apply sterile cover.  Seek medical attention


Inhalation
Inhalation of hot vapours may cause irritation to upper respiratory tract and coughing.  Move to fresh air.  If symptoms persist consult medical advice.

Ingestion
Rinse mouth if contaminated.  Do not induce vomiting.  Seek medical



advice.

Advice to physician

see above.

______________________________________________________________________________________________________
5)
Fire-fighting measures:


Suitable extinguishing media

CO2 , foam, dry chemical powder, sand, water fog

Extinguishing media which must 

water stick jets

not be used for safety reasons


Special exposure hazards arising 

incomplete combustion produces fumes,

 
from the substance, its combustion

flue gases, carbon monoxide


products, resulting gases


Special protective equipment

breathing protection independent of the




ambient air


Additional information

apply cold water in order to cool containers and 



environment exposed to danger.

_
______________________________________________________________________________________________________
6)
Accidental release measures:


Personal precautions

Wear protective clothing.  Keep persons not involved in rescue away

Environmental precautions
solid 
)
keep away from drains and surface 



liquid 
)
water


Method for cleaning up
solid
remove mechanically 



liquid
contain the product, allow to cool and remove mechanically.  Alternatively, absorb the liquid product with sand and then remove mechanically

Additional instructions
solid
not applicable



liquid
inform authorities in the case of leakage of large amounts

______________________________________________________________________________________________________
7)
Handling and Storage:


Handling

there are no special regulations


Instructions for safe handling
solid
usual handling of solid transport goods



liquid
usual precautions for handling hot fluids.   



Use standard industrial hygiene measures for handling chemical substances

Instructions for prevention of fire
solid
none


and explosion
liquid
prevent aerosol generation during pumping



powder 
danger (of explosion) adopt measures to prevent dust-explosion; (see point 9)


Storage

Requirements for storage rooms
slabs/ ) 
store under cool, dry and light protected


and containers
powder/ )
conditions



pastilles )




liquid
storage tanks have to be installed and 


managed according to official regulations.


Information on storage concerning

liquid material is not allowed to contain water 


incompatible substances

at temperatures above 100°C (delay in boiling)


Additional information

see point 10 = stability and reactivity.

______________________________________________________________________________________________________​​​​_






8)
Exposure controls/Personal protection:


Exposure limits

Ensure good ventilation when processing at elevated temperatures.


Occupational Exposure Limits - U.K. - Paraffin Wax fume 


Long term exposure limit 
(  8 hour TWA)
2mg/M3

Short term exposure limit
(10 minutes)
6mg/M3

Personal protection


Respiratory protection
solid
none



liquid
work in well ventilated rooms


Hand protection
solid
none



liquid
wear rubber or leather gloves


Eye protection
solid
none



liquid
wear safety goggles


Body protection
solid
none



liquid
wear protective clothing

______________________________________________________________________________________________________
9)
Physical Properties:


Physical state:

At 20°C - waxy solid (slabs, pastilles, powder).  

Above the congealing point, liquid.


Colour:

Whitish


Odour:

Nearly odourless


Congealing Point:

52 - 54°C                    DIN-ISO 2207


Flash Point:

220 °C.   DIN-ISO 2592


Autoflammability:

Not determined


Explosive Properties:


In powder form, may form an explosive 





atmosphere 

Vapour Pressure (20°C)

No data available, negligible

Density (20°C)

Approximately 0.73 – 0.84 g/cm3

Solubility in water (20°C)

Less than 10 - 2  g/1


        in white spirit (80°C)

Miscible


pH - value

not applicable
______________________________________________________________________________________________________
10)
Stability and reactivity:


Conditions to avoid
liquid
prolonged storage 20°C above congealing point 


may interfere with quality


Materials to avoid
solid/  )
avoid contact with strong oxidising agents




liquid  )


Hazardous decomposition products

flue gas, carbon monoxide, aldehydes in the  


case of incomplete combustion


Thermal decomposition

Greater than 180°C (DSC 10°C/min  




CrNi-crucible)

______________________________________________________________________________________________________
11)
Toxicological information:


Toxicological information

Summary


there is no evidence of chronic toxic effects to 





experimental animals of paraffin wax


Acute toxicity

oral LD50  rat : greater than 3750 mg/kg





dermal LD50 rabbit: >4 ml/kg

Mutagenicity

no evidence has been found


Carcinogenicity

no evidence has been found

Information on irritative effects

Summary


there is no evidence of irritative effects to skin 



from the long-term application as ingredient in 



skin products




Eye:
non-irritating




Skin:
non-irritating




Swallowing:
harmless (not toxic, see oral LD50 - value)

_______________________________________________________________________________________________________

12)
Ecological Information:


No negative ecological effects are known at present.  Mechanical separation in a sewage plant is possible.


Mobility

Spillage’s are unlikely to penetrate the soil.


Persistence and degradability


These products are inherently biodegradable.


There is no evidence to suggest bioaccumulation will occur.  Some bacteria and fungi reproduce themselves on paraffin wax using it as carbon source in aerobic conditions.


BOD 35 days (C6-C31: 66-88% TOD 


BOD 28 days (C19-C47: 78-84% TOD


BOD 84 days (C19-C47: 85-98% TOD


Bioaccumulative potential

logKow: >6 (estimated)


Potentially bioaccumulative but practically insoluble in water, furthermore hydrocarbons having high molecular weight are too large to be absorbed through biological membranes

_______________________________________________________________________________________________________

13)
Disposal Considerations:


Where possible, arrange for product to be recycled.  Dispose of via an authorised/licensed waste disposal contractor in accordance with local regulations.  Incineration may be carried out under controlled conditions, or dispose of at landfill provided that local regulations are met.  Do not dispose of near ponds, ditches, down drains or onto soil.  Dispose of container in the same way as product.
______________________________________________________________________________________________________
14)
Transport Information:


Not classified as hazardous for transport  (ADR, RID, UN, IATA/ICAO/IMO).


(Class 9 if liquid [over 80°C] for sea freight.)

______________________________________________________________________________________________________
15)
Regulatory Information:


Labeling information:

S2: Keep out of reach of children


S16: Keep away from ignition sources – do not smoke

S62: If swallowed do not induce vomiting: seek medical advice immediately and show this container or label.
Other: These products conform to the FDA and BGA regulations governing products intended for food contact.
______________________________________________________________________________________________________
16)
Other Information:

This advice is given by Meade-King, Robinson and Co Limited who accept no legal liability for it except otherwise provided by law.  The information contained herein is based on the present state of our knowledge and is intended to describe our products from the point of view of safety requirements.  It should not therefore be construed as guaranteeing specific properties.

The information contained in this document does not constitute a risk assessment and should not replace the user’s own assessment of risks as required by other health and safety legislation
______________________________________________________________________________________________________
